FRESH WATER WORK

|  |  |  |
| --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870**Job Title:** **Site Address:**  | **Date:** **Page:** 1 of 2 **SWMS No:** 08 | **New****Revised** |
| **Principal:**  | **Supervisor:** Ian Loccisano | **Approved by:** Ian Loccisano |
| **Required Personal Protective Equipment:** As required for tasks being carried out |
| TASK | **POTENTIAL HAZARDS** | **ACTION OR PROCEDURE** | **RESPONSIBILITY** |
| Working over fresh water | Drowning | Ensure lockout in place on butterfly valves above work area before entry into work area | Supervisor |
| Conduct risk assessment of potential for inundation from Barron River in consultation with Sun Water & SCL before working in draft tube & tail race | Supervisor |
| Where identified as necessary, place edge protection to prevent fall into water | Supervisor |
| For work in draft tube & tail race ensure baulk gate controls in place | Supervisor |
| Follow of system as per risk assessment | All workers |
| No person to work in isolation | All workers |
| Where practicable water pumped from below work area | Supervisor |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7