HEIGHTS > 2.0m – EDGE PROTECTION

|  |  |  |
| --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870**Job Title:** **Site Address:**  | **Date:** **Page:** 1 of 2 **SWMS No:** 11 | **New****Revised** |
| **Principal:**  | **Supervisor:** Ian Loccisano | **Approved by:** Ian Loccisano |
| **Required Personal Protective Equipment:** Soft sole safety shoes when working on a roof, otherwise safety boots. Other PPE as required by site safety rules |
| **TASK** | **POTENTIAL HAZARDS** | **ACTION OR PROCEDURE** | **RESPONSIBILITY** |
| Work at heights over 2.0m | General | All persons instructed in use of edge protection | Supervisor |
| Daily monitoring for compliance with WH&S Regulation | Supervisor |
| Fall | Edge protection components inspected & in good order | User |
| Edge protection installed in accordance with manufacturer’s instructions including top rail, mid rail & toe board | User |
| Loss of foothold | Soft sole safety shoes when working on a roof, otherwise safety boots | Supervisor |
| Injury after fall | No protruding objects below | User |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7