HEIGHTS > 2.0m – SCAFFOLD

|  |  |  |
| --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870**Job Title:** **Site Address:**  | **Date:** **Page:** 1 of 2 **SWMS No:** 17 | **New****Revised** |
| **Principal:**  | **Supervisor:** Ian Loccisano | **Approved by:** Ian Loccisano |
| **Required Personal Protective Equipment:** As per site requirements |
| **TASK** | **POTENTIAL HAZARDS** | **ACTION OR PROCEDURE** | **RESPONSIBILITY** |
| Work at heights over 2.0m | General | All persons instructed in use of scaffold | Supervisor |
| Daily periodical monitoring for compliance with WH&S Regulation | Supervisor |
| Scaffold hand over certificate completed if appropriate | Supervisor |
| Scaffold erected by licensed scaffolder | Supervisor |
| Fall | Scaffold erected to plan including:Full decking, handrail, mid rail, toe board, access & sole plates | Licensed scaffolder |
| Scaffold tag provided to indicate status | Supervisor |
| Scaffold maintained in good working order & recorded | Supervisor |
| Scaffold barricaded off to prevent access after hours | User |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7