HEIGHTS > 2.0m – LADDER

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870  **Job Title:**  **Site Address:** | | | | **Date:**  **Page:** 1 of 2 **SWMS No:** 16 | | **New**  **Revised** |
| **Principal:** | | **Supervisor:** Ian Loccisano | | **Approved by:** Ian Loccisano | | |
| **Required Personal Protective Equipment:** Pole strap or harness system, safety footwear appropriate to task | | | | | | |
| **TASK** | **POTENTIAL HAZARDS** | | **ACTION OR PROCEDURE** | | **RESPONSIBILITY** | |
| Work at heights over 2.0m | General | | All persons instructed in use of ladder | | Supervisor | |
| Daily periodical monitoring for compliance with WH&S Regulation | | Supervisor | |
| Fall | | Ladder marked with load rating of at least 120kg and industrial type | | User | |
| Extension ladder not to exceed 7.5m except for use in a confined space | | User | |
| Ladder angle between 70° & 80° or 1:4 except for use in a confined space | | User | |
| Ladder placed on stable surface | | User | |
| Ladder securely anchored top & bottom | | User | |
| Three point contact maintained at all times | | User | |
| Use of a ladder strap or fall arrest harness system | | User | |
| Loss of foot hold | | Safety footwear appropriate to the task | | User | |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7