HEIGHTS > 2.0m – SCAFFOLD

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870  **Job Title:**  **Site Address:** | | | | **Date:**  **Page:** 1 of 2 **SWMS No:** 17 | | **New**  **Revised** |
| **Principal:** | | **Supervisor:** Ian Loccisano | | **Approved by:** Ian Loccisano | | |
| **Required Personal Protective Equipment:** As per site requirements | | | | | | |
| **TASK** | **POTENTIAL HAZARDS** | | **ACTION OR PROCEDURE** | | **RESPONSIBILITY** | |
| Work at heights over 2.0m | General | | All persons instructed in use of scaffold | | Supervisor | |
| Daily periodical monitoring for compliance with WH&S Regulation | | Supervisor | |
| Scaffold hand over certificate completed if appropriate | | Supervisor | |
| Scaffold erected by licensed scaffolder | | Supervisor | |
| Fall | | Scaffold erected to plan including:  Full decking, handrail, mid rail, toe board, access & sole plates | | Licensed scaffolder | |
| Scaffold tag provided to indicate status | | Supervisor | |
| Scaffold maintained in good working order & recorded | | Supervisor | |
| Scaffold barricaded off to prevent access after hours | | User | |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7