TRENCH > 1.5m DEEP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870  **Job Title:**  **Site Address:** | | | | **Date:**  **Page:** 1 of 3 **SWMS No:** 24 | | **New**  **Revised** |
| **Principal:** | | **Supervisor:** Ian Loccasino | | **Approved by:** Ian Loccisano | | |
| **Required Personal Protective Equipment:** Safety boots, high visibility vest or shirt. Safety helmet | | | | | | |
| **TASK** | **POTENTIAL HAZARDS** | | **ACTION OR PROCEDURE** | | **RESPONSIBILITY** | |
| Preplanning | General | | All persons inducted as per SWMS | | Supervisor | |
| Services | | Refer SWMS Underground Services | | Competent person | |
| Permit to excavate issued where required | | Competent person | |
| Person entering trench | Access & egress falls | | Ladder provided & secured every 9m of trench occupied | | Competent person | |
| Atmospheric quality | | Check for contaminated atmosphere | | Competent person | |
| Refer SWMS Confined Space if atmosphere contaminated | | Supervisor | |
| Falling objects | | Wear safety helmet | | All workers | |
| Water in trench | | Dewater as required. Drawdown rate not causing leaching of fine soil particles resulting in undermining | | All workers | |
| Collapse of trench | | No vertical height greater than 1.5m | | Competent person | |

|  |  |  |  |
| --- | --- | --- | --- |
| **TASK** | **POTENTIAL HAZARDS** | **ACTION OR PROCEDURE** | **RESPONSIBILITY** |
| Person entering trench | Collapse of trench | Assess ground stability for unstable soil, underground water table, adjacent trenches, vibration from plant | Competent person |
| Consider option of batter/bench/shore or combination of above | Competent person |
| Tick applicable control measure  Batter at 1:1 slope  Bench at theoretical 1:1 slope  Shore trench (proprietary product)  Combination of batter/bench/shore  Certification by a geotechnical engineer where not battered, benched or shored | Competent person |
| Check for surcharge on trench walls | Competent person |
| Material falling into trench | Spoil material clear of trench sides | Operator digging trench |
| Persons in trench to withdraw for installing pipes by crane or placement of backfill | Operator placing backfill |
| Shoring (if used) protrudes 300mm above natural surface | Competent person |
| Persons falling into trench | Backfill trench as laying pipe | Competent person |
| Open trench not left unattended unless barricaded, plated over or sentry posted | Competent person |
| All hazards | Daily periodical monitoring of activity | Supervisor |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7