HEIGHTS > 2.0m – EDGE PROTECTION

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870  **Job Title:**  **Site Address:** | | | | **Date:**  **Page:** 1 of 2 **SWMS No:** 11 | | **New**  **Revised** |
| **Principal:** | | **Supervisor:** Ian Loccisano | | **Approved by:** Ian Loccisano | | |
| **Required Personal Protective Equipment:** Soft sole safety shoes when working on a roof, otherwise safety boots. Other PPE as required by site safety rules | | | | | | |
| **TASK** | **POTENTIAL HAZARDS** | | **ACTION OR PROCEDURE** | | **RESPONSIBILITY** | |
| Work at heights over 2.0m | General | | All persons instructed in use of edge protection | | Supervisor | |
| Daily monitoring for compliance with WH&S Regulation | | Supervisor | |
| Fall | | Edge protection components inspected & in good order | | User | |
| Edge protection installed in accordance with manufacturer’s instructions including top rail, mid rail & toe board | | User | |
| Loss of foothold | | Soft sole safety shoes when working on a roof, otherwise safety boots | | Supervisor | |
| Injury after fall | | No protruding objects below | | User | |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7