HEIGHTS > 2.0m – HARNESS & DROP LINE

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870  **Job Title:**  **Site Address:** | | | | **Date:**  **Page:** 1 of 2 **SWMS No:** 13 | | **New**  **Revised** |
| **Principal:** | | **Supervisor:** Ian Loccisano | | **Approved by:** Ian Loccisano | | |
| **Required Personal Protective Equipment:** Harness, drop line, safety footwear appropriate to task as per risk assessment | | | | | | |
| TASK | **POTENTIAL HAZARDS** | | **ACTION OR PROCEDURE** | | **RESPONSIBILITY** | |
| Work at heights over 2.0m | General | | All persons instructed in use of harness & drop line | | Supervisor | |
| Daily periodical monitoring for compliance with WH&S Regulation | | Supervisor | |
| Fall | | Drop line constructed of 16mm silver rope | | User | |
| Drop line has a stop spliced in the tail | | User | |
| Rope adjusted in good working order | | User | |
| Drop line securely anchored | | User | |
| Harness fitted correctly (buddy system) | | User | |
| Harness inspected & in good condition | | User | |
| Harness secured to rope adjuster by karabiner | | User | |

|  |  |  |  |
| --- | --- | --- | --- |
| TASK | **POTENTIAL HAZARDS** | **ACTION OR PROCEDURE** | **RESPONSIBILITY** |
| Work at heights over 2.0m | Loss of foot hold | Risk assessment to determine appropriate footwear or surface to be laid if applicable (rubber matting) | Supervisor |
| Injury after fall | No protruding objects below | User |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7