HEIGHTS > 2.0m – HARNESS & STATIC LINE

|  |  |  |
| --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870**Job Title:** **Site Address:**  | **Date:** **Page:** 1 of 2 **SWMS No:** 14 | **New****Revised** |
| **Principal:**  | **Supervisor:** Ian Loccisano | **Approved by:** Ian Loccisano |
| **Required Personal Protective Equipment:** Harness, static line, lanyard, footwear appropriate to task as per risk assessment |
| **TASK** | **POTENTIAL HAZARDS** | **ACTION OR PROCEDURE** | **RESPONSIBILITY** |
| Work at heights over 2.0m | General | All persons instructed in use of harness and static line | Supervisor |
| Daily periodical monitoring for compliance with WH&S Regulation  | Supervisor |
| Fall | Static line inspected and in good order | User |
| Static line securely anchored and tensioned | User |
| Lanyard inspected and in good order | User |
| Harness inspected and in good condition | User |
| Lanyard secured to static line by karabiner | User |
| Harness secured to lanyard by karabiner | User |
| Harness fitted correctly and comfortable | User |
| **TASK** | **POTENTIAL HAZARDS** | **ACTION OR PROCEDURE** | **RESPONSIBILITY** |
| Work at heights over 2.0m | Loss of Foothold | Risk assessment to determine appropriate footwear for task | Supervisor |
| Injury after Fall | No protruding objects below | User |
| Retrieval method in place | Supervisor |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7