HEIGHTS > 2.0m – HARNESS & DROP LINE

|  |  |  |
| --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870**Job Title:** **Site Address:**  | **Date:** **Page:** 1 of 2 **SWMS No:** 13 | **New****Revised** |
| **Principal:**  | **Supervisor:** Ian Loccisano | **Approved by:** Ian Loccisano |
| **Required Personal Protective Equipment:** Harness, drop line, safety footwear appropriate to task as per risk assessment |
| TASK | **POTENTIAL HAZARDS** | **ACTION OR PROCEDURE** | **RESPONSIBILITY** |
| Work at heights over 2.0m  | General | All persons instructed in use of harness & drop line | Supervisor |
| Daily periodical monitoring for compliance with WH&S Regulation | Supervisor |
| Fall | Drop line constructed of 16mm silver rope | User |
| Drop line has a stop spliced in the tail | User |
| Rope adjusted in good working order | User |
| Drop line securely anchored | User |
| Harness fitted correctly (buddy system) | User |
| Harness inspected & in good condition | User |
| Harness secured to rope adjuster by karabiner | User |

|  |  |  |  |
| --- | --- | --- | --- |
| TASK | **POTENTIAL HAZARDS** | **ACTION OR PROCEDURE** | **RESPONSIBILITY** |
| Work at heights over 2.0m | Loss of foot hold | Risk assessment to determine appropriate footwear or surface to be laid if applicable (rubber matting) | Supervisor |
| Injury after fall | No protruding objects below | User |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7