HEIGHTS > 2.0m – HARNESS & STATIC LINE

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870  **Job Title:**  **Site Address:** | | | | **Date:**  **Page:** 1 of 2 **SWMS No:** 14 | | **New**  **Revised** |
| **Principal:** | | **Supervisor:** Ian Loccisano | | **Approved by:** Ian Loccisano | | |
| **Required Personal Protective Equipment:** Harness, static line, lanyard, footwear appropriate to task as per risk assessment | | | | | | |
| **TASK** | **POTENTIAL HAZARDS** | | **ACTION OR PROCEDURE** | | **RESPONSIBILITY** | |
| Work at heights over 2.0m | General | | All persons instructed in use of harness and static line | | Supervisor | |
| Daily periodical monitoring for compliance with WH&S Regulation | | Supervisor | |
| Fall | | Static line inspected and in good order | | User | |
| Static line securely anchored and tensioned | | User | |
| Lanyard inspected and in good order | | User | |
| Harness inspected and in good condition | | User | |
| Lanyard secured to static line by karabiner | | User | |
| Harness secured to lanyard by karabiner | | User | |
| Harness fitted correctly and comfortable | | User | |
| **TASK** | **POTENTIAL HAZARDS** | | **ACTION OR PROCEDURE** | | **RESPONSIBILITY** | |
| Work at heights over 2.0m | Loss of Foothold | | Risk assessment to determine appropriate footwear for task | | Supervisor | |
| Injury after Fall | | No protruding objects below | | User | |
| Retrieval method in place | | Supervisor | |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7