HEIGHTS > 2.0m – HARNESS, TRIPOD & HAND WINCH

|  |  |  |
| --- | --- | --- |
| **PCBU Address:** Lot 3, Redlynch Connector Road, Redlynch 4870**Job Title:** **Site Address:**  | **Date:** **Page:** 1 of 2 **SWMS No:** 15 | **New****Revised** |
| **Principal:**  | **Supervisor:** Ian Loccisano | **Approved by:** Ian Loccisano |
| **Required Personal Protective Equipment:** Harness, spreader bar, safety footwear appropriate to task |
| **TASK** | **POTENTIAL HAZARDS** | **ACTION OR PROCEDURE** | **RESPONSIBILITY** |
| Work at heights over 2.0m | General | All persons instructed in use of tripod/davit, winch & harness | Supervisor |
| Daily periodical monitoring for compliance with WH&S Regulation | Supervisor |
| Fall | Hand winch fitted to tripod/davit | Supervisor |
| Tripod/davit secured in position | Supervisor |
| Winch operator in place | Supervisor |
| Harness fitted to persons correctly (use buddy system) | User |
| Spreader bar used if required | User |
| Winch line connected to harness or spreader bar as required | User |
| User remains connected to winch line | User |
| Loss of foot hold | Safety footwear appropriate to the task | User |
| Injury after fall | No protruding items below | User |

Risk assessment based on all procedures being in place

**Risk Assessment Matrix**



**Likelihood:** Very unlikely **Consequences:** Minor **Risk score:** 7